**Product Card For**: SKU# RPOSPF Reclaimed Pub Oak Skip Planed Face

**Price:**

**Species:** White Oak, Red Oak some mixed Ash or Maple

**Thickness:** ¾” **Width:** 3” – 11” **Length:** 3’ – 12’ and longer

**Surface Texture:** Rough saw marks, some weathering and checking with portion of smooth patches – these are high spots in the material that were planed down.

**Color:** Light to Brown Tans to Dark Brown and Black

**Hardness:** Very Hard and Durable

**Uses:**

**Descriptions:** This material comes from Reclaimed Barn Beams that were re-sawn, center of beams -not outer Skins, into boards.

**Lead Time:** 3-4 weeks from date of order, call to check stock.

**Origin of Material:** This material comes from Barns and Structures from NY and PA.

**Installation:** This flooring has a standard T/G, so flooring nails or staples can be used. Glue down and nails are good methods to install over wood. Good quality glue can be used to install over concrete. Can install over radiant heat but, allow more time for floor to acclimate

**Finishing Preparation:** After installation, this may or may not require light screening, depending on how much texture is desired, just fill nail/knot holes with filler fill check. If desired, lightly sand just areas that were filled. Quality wood filler like Mohawk Wood Putty should be used. Add Stain to areas that were filled to proper color.

**Finish:** Use a quality Pre-Stain Sealer so even stain absorption is achieved. Using quality stains like Mohawk Wiping Stain. Install a Sealer Coat and apply 3 coats of quality Top Coat. If dry time is not a big issue, we recommend a quality Tung Oil Finish like a Water Lox Marine Grade Tung Oil, a traditional finish that has been used for over 100 years.