**Product Card For**: SKU# ROA

**Price:**

**Species:** White Oak, Red Oak some mixed Ash or Maple

**Thickness:** ¾” **Width:** 3” – 11” **Length:** 3’ – 12’ and longer

**Surface Texture:** Smooth Surface with some nail knot holes and surface checking that need to be filled

**Color:** Light Tans slight reddish tint to Dark Tans

**Hardness:** Very Hard and Durable

**Uses:** Great material for Floors – can also be a Wall or Ceiling

**Descriptions:** This material comes from Reclaimed Barn Beams that were re-sawn, center of beams -not outer Skins, into boards.

**Lead Time:** 2-3 weeks from date of order. Call to check stock. Good chance of having this material in stock.

**Origin of Material:** This material comes from Barns and Structures from NY and PA.

**Installation:** This flooring has a standard T/G, so flooring nails or staples can be used. Glue down and nails are good methods to install over wood. Good quality glue can be used to install over concrete. Can install over radiant heat but, allow more time for floor to acclimate

**Pre-Finish:** After installation this floor will not be sanded, just fill nail knot holes with fill checking, if desired, and lightly sand just areas that were filled with quality wood filler like Mohawk Wood Putty