Product Card For: Reclaimed Pub Oak Original Face

**Species:** White Oak, Red Oak some mixed Ash or Maple

**Thickness:** ¾” **Width:** 3” – 11” **Length:** 3’ – 12’ and longer

**Surface Texture:** Rough Saw Marks, Some weathering and Checking

**Color:** Light to Brown Tans to Dark Brown and Black

**Hardness:** Very Hard and Durable

**Uses:** Restaurants

**Descriptions:** This material comes from surfaces of Barn Beams floor planks and dividing will be Barn Stalls.

**Lead Time:** 2-3 weeks from date of order. Call to check stock.

**Origin of Material:** This material comes from Barns and Structures from NY and PA.

**Installation:** This flooring has a standard T/G, so flooring nails or staples can be used. Glue down and nails are good methods to install over wood. Good quality glue can be used to install over concrete. Can install over radiant heat but, allow more time for floor to acclimate

**Pre- Finish:** After installation, this floor will not be sanded, just fill nail/knot holes with fill checking if desired and lightly sand just areas that were filled. Quality wood filler like Mohawk Wood Putty